{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["EPC CPC RER Calc","Lighting"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":3,"defined_names":80,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EPC CPC RER Calc","index":0,"n_rows":121,"n_cols":28,"rows_kept":121,"cut":false,"hidden":false,"merged":[[83,10,83,11],[0,0,0,3],[2,3,2,6],[54,3,54,4],[12,3,16,3],[17,3,17,4],[45,3,45,4],[46,3,46,4],[53,3,53,4],[28,3,33,3],[4,0,4,7],[7,0,7,7],[80,3,80,4],[61,3,61,4],[69,3,71,3],[73,3,73,4],[109,3,113,3],[100,3,100,4],[81,3,81,4],[82,3,82,4],[107,4,107,6],[104,5,104,6],[3,0,3,1],[74,3,74,4],[93,3,93,4],[92,3,92,4],[95,3,95,4],[94,3,94,4]]}
["Interim NZEB Specification Tool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fuel",null,null,null,null,"Yes"]
["VERSION 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electricity",2.08,0.40899999999999997,null,null,"No"]
["Publication Date: Q4 2017",null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mains Gas",1.1000000000000001,0.20300000000000001]
["Note: Electrical Primary Energy Factor updated to 2.08 and CO2 emissions 0.409 kg/kWh",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LPG",1.1000000000000001,0.23200000000000001]
["1. General information",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oil",1.1000000000000001,0.27200000000000002]
["Public Body:"," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"House coal/ Anthracite",1.1000000000000001,0.36099999999999999]
["Building Address:"," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dual Fuel",1.1000000000000001,0.28899999999999998]
["2. Assessor Details",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Smokeless Fuel",1.2,0.39200000000000002]
["Assessor Name:"," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biomass",1.1000000000000001,2.5000000000000001E-2]
["Assessor Number:"," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas",1.1000000000000001,2.5000000000000001E-2]
["3. Reference Building Data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waste Heat",1.05,1.7999999999999999E-2]
[null,"Actual Energy Use:",null,"Guidance Note:","Fuel:","Primary Energy:","CO2 Emissions:"]
["Heating Energy",0,"kWh/m2/yr","Values are taken from the actual energy use for the manually created Reference Building","Mains Gas",{"$f":"B13*J13","v":0},{"$f":"B13*K13","v":0},null,null,{"$f":"VLOOKUP(E13,$W$2:$Y$9,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(E13,$W$2:$Y$9,3,)","v":0.20300000000000001}]
["Cooling Energy",0,"kWh/m2/yr",null,"Electricity",{"$f":"B14*J14","v":0},{"$f":"B14*K14","v":0},null,null,{"$f":"VLOOKUP(E14,$W$2:$Y$9,2,)","v":2.08},{"$f":"VLOOKUP(E14,$W$2:$Y$9,3,)","v":0.40899999999999997}]
["Auxiliary Energy",0,"kWh/m2/yr",null,"Electricity",0,0,null,null,{"$f":"VLOOKUP(E15,$W$2:$Y$9,2,)","v":2.08},{"$f":"VLOOKUP(E15,$W$2:$Y$9,3,)","v":0.40899999999999997}]
["Lighting Energy",0,"kWh/m2/yr",null,"Electricity",0,0,null,null,{"$f":"VLOOKUP(E16,$W$2:$Y$9,2,)","v":2.08},{"$f":"VLOOKUP(E16,$W$2:$Y$9,3,)","v":0.40899999999999997}]
["Hot Water Energy",0,"kWh/m2/yr",null,"Mains Gas",0,0,null,null,{"$f":"VLOOKUP(E17,$W$2:$Y$9,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(E17,$W$2:$Y$9,3,)","v":0.20300000000000001}]
[null,null,null,"Reference Building without Renewable Contribution",null,{"$f":"SUM(F13:F17)","v":0},{"$f":"SUM(G13:G17)","v":0}]
["Renewable Energy Ratio",{"$f":"20%","v":0.2}]
["Epren Primary Renewable Energy  required to meet RER",{"$f":"F18*B19","v":0},"kWh/m2/yr"]
["Area of Building",0,"m2"]
["Estimated apeture area of photovoltaic \n(based on south facing panels at 30 degree angle with no overshading)",{"$f":"(B20/X2)*B21/(1076*15%*75%)","v":0},"m2"]
[]
["Reference Building Primary Energy Use",{"$f":"F18-B20","v":0},"kWh/m2/yr"]
["Reference Building Carbon Emissions",{"$f":"G18-((B20*Y2)/X2)","v":0},"kgCO2/m2/yr"]
[]
["4. Actual Building Data"]
[null,"Actual Energy Use:",null,"Guidance Note:","Fuel:","Primary Energy:","CO2 Emissions:"]
["Heating Energy",0,"kWh/m2/yr","Values are taken from the actual energy use for the Actual Building","Mains Gas",{"$f":"B29*J29","v":0},{"$f":"B29*K29","v":0},null,null,{"$f":"VLOOKUP(E29,$W$2:$Y$11,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(E29,$W$2:$Y$11,3,)","v":0.20300000000000001}]
["Cooling Energy",0,"kWh/m2/yr",null,"Electricity",{"$f":"B30*J30","v":0},{"$f":"B30*K30","v":0},null,null,2.08,0.40899999999999997]
["Auxiliary Energy",0,"kWh/m2/yr",null,"Electricity",0,0,null,null,2.08,0.40899999999999997]
["Lighting Energy",0,"kWh/m2/yr",null,"Electricity",0,0,null,null,2.08,0.40899999999999997]
["Hot Water Energy",0,"kWh/m2/yr",null,"Mains Gas",0,0,null,null,1.1000000000000001,0.20300000000000001]
["Alternate Fuel",0,"kWh/m2/yr",null,"Electricity",{"$f":"B34*J34","v":0},{"$f":"B34*K34","v":0},null,null,2.08,0.40899999999999997]
[null,null,null,null,null,{"$f":"SUM(F29:F34)","v":0},{"$f":"SUM(G29:G34)","v":0}]
[null,"Installed Renewable Energy"]
["Photovoltaic","Yes"," "]
["Wind Energy","Yes"," "]
["Solar Panel","Yes"," "]
["Biomass/ Biogas","Yes"," "]
["Combined Heat and Power","Yes"," "]
["Heat Pump Technology","Yes"," "]
[null,null,null," "]
["Photovoltaic"]
[null,"Energy Contribution taken from XXX_sim file",null,null,null,"Primary Energy Factor","CO2 Emissions"]
["Photovoltaic",0,"kWh/m2/yr","Photovoltaic Used on Site",null,{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}," "]
["% of Photovoltaic used on site",1," ","Photovoltaic Exported Off Site",null,{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}]
[]
["Primary Energy from Photovoltaic",{"$f":"B46*B47*F46+B46*(1-B47)*F47","v":0},"kWh/m2/yr"]
["Carbon Emissions from Photovoltaic",{"$f":"B46*B47*G46+B46*(1-B47)*G47","v":0},"kgCO2/m2/yr"]
[]
["Wind Energy"]
[null,"Energy Contribution taken from XXX_sim file",null,null,null,"Primary Energy Factor","CO2 Emissions"]
["Wind Energy",0,"kWh/m2/yr","Wind Energy Used on Site",null,{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}]
["% of Wind Energy used on site",1," ","Wind Energy Exported Off Site",null,{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}]
[]
["Primary Energy from Photovoltaic",{"$f":"B54*B55*F54+B54*(1-B55)*F55","v":0},"kWh/m2/yr"]
["Carbon Emissions from Photovoltaic",{"$f":"B54*B55*G54+B54*(1-B55)*G55","v":0},"kgCO2/m2/yr"]
[]
["Solar Panel"]
[null,"Energy Contribution taken from XXX_sim file",null,null,null,"Primary Energy Factor","CO2 Emissions"]
["SES",0,"MJ/m2","Solar Panel",null,{"$f":"J33","v":1.1000000000000001},{"$f":"K33","v":0.20300000000000001}," "]
["Seasonal Efficiency of Heat Source",0.91]
["Primary Energy from Solar Panels",{"$f":"(B62/3.6/B63)*F62","v":0},"kWh/m2/yr",null,null,null,null," "]
["Carbon Emissions from Solar Panels",{"$f":"(B62/3.6/B63)*G62","v":0},"kgCO2/m2/yr"]
[]
[]
["Biomass/ Biogas"]
[null,"Based on Design Calculation",null,"Guidance Note:",null," "," "," ",null," "," "]
["% of Delivered Heating provided by Biomass/ Biogas",0,null,"Refer to Guidance Document for calculation of %",null,"Primary Energy Factor","CO2 Emissions",null,null," "," "]
["% of Delivered Hot Water provided by Biomass/ Biogas",0,null,null,"Biomass/ Biogas",{"$f":"X9","v":1.1000000000000001},{"$f":"Y9","v":2.5000000000000001E-2}]
["Fuel of Other System","Mains Gas"," ",null,{"$f":"B72","v":"Mains Gas"},{"$f":"VLOOKUP(B72,$W$2:$Y$11,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(B72,$W$2:$Y$11,3,)","v":0.20300000000000001},null,null," "," "]
[null,null,null,null,null," ",null,null,null," "," "]
["Primary Energy from Biomass",{"$f":"((B29*B70)+(B33*B71))*F71","v":0},"kWh/m2/yr","Primary Energy Use from Htg & DHW",null,{"$f":"((B29*B70)+(B33*B71))*F71+(B29*(100%-B70)+(B33*(100%-B71)))*F72","v":0},"kWh/m2/yr"]
["Carbon Emissions from Biomass",{"$f":"((B29*B70)+(B33*B71))*G71","v":0},"kgCO2/m2/yr","CO2 from Htg & DHW",null,{"$f":"((B29*B70)+(B33*B71))*G71+(B29*(100%-B70)+(B33*(100%-B71)))*G72","v":0},"kgCO2/m2/yr"]
[]
[null,null,null,null,null," "]
[null,null,null,null,null,null,null,null," "]
["Combined Heat and Power",null,null,null,null,null,null,null," "]
[null,"Energy Contribution taken from XXX_sim file",null,null,null,null,null,null," "]
["CHP_All",136.36000000000001,"kWh/m2","Heating and Hot Water",null,{"$f":"B81*B83","v":74.998000000000019},"kWh/m2"]
["Electrical Efficiency of CHP",0.3," ","Electrical",null,{"$f":"B81*B82","v":40.908000000000001},"kWh/m2"]
["Thermal Efficiency of CHP",0.55000000000000004," ",null,null," "," "]
["CHP Fuel","Mains Gas",null,null,null,"Primary Energy Factor","CO2 Emissions",null,null,{"$f":"IF(B84=\"Biomass\",0.75,0.86)","v":0.86},"min boiler efficiency based on fuel"]
["Renewable Primary Energy from CHP",{"$f":"IF(B84=\"Biogas\",F81*((F86/J84)+B82*F85/(B83)),F81*((F86/J84)+B82*F85/(B83)-(F86/B83)))","v":31.020314418604645},"kWh/m2/yr",null,"Electricity",{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}," "]
[null,null,null,null,{"$f":"B84","v":"Mains Gas"},{"$f":"VLOOKUP(B84,$W$2:$Y$11,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(B84,$W$2:$Y$11,3,)","v":0.20300000000000001}]
[null," "]
[null,null,null,null,null,null," "]
["Heat Pump"]
[null,"Based on Design Calculation",null,null,null,"Primary Energy Factor","CO2 Emissions"]
["% of Heating provided by Heat Pump",0.5,null,null,"Electricity",{"$f":"X2","v":2.08},{"$f":"Y2","v":0.40899999999999997}]
["Efficiency of Heat Pump for Heating",4.5,null,null,{"$f":"B95","v":"Mains Gas"},{"$f":"VLOOKUP(E92,$W$2:$Y$11,2,)","v":1.1000000000000001},{"$f":"VLOOKUP(E92,$W$2:$Y$11,3,)","v":0.20300000000000001}]
["% of Hot Water provided by Heat Pump",1," ","Bivalent Seasonal Efficiency for Heating",null,{"$f":"F91/((F91/B92*B91)+(F92/B96*(1-B91)))","v":2.4895072192669665}]
["Efficiency of Heat Pump for Hot Water",2," ","Bivalent Seasonal Efficiency for Hot Water",null,{"$f":"F91/((F91/B94*B93)+(F92/B96*(1-B93)))","v":2}," "]
["Fuel of Other System","Mains Gas",null,"Heating from Heat Pump",null,{"$f":"B29*F93*B91/B92","v":0},"kWh/m2"]
["Seasonal Efficiency of Heat Source",0.91,null,"Hot Water from Heat Pump",null,{"$f":"B33*F94*B93/B94","v":0},"kWh/m2"]
[]
["Renewable Primary Energy from Heat Pump",{"$f":"IF(AND(B91>0,B92>208%),(B92*(1.1/0.86)-208%)*F95,0)+IF(AND(B93>0,B94>208%),(B94*(1.1/0.86)-208%)*F96,0)","v":0},"kWh/m2/yr"," "]
[null,null,null,null,null,null," "]
[]
[null,null,null,"Results from SBEM",null,{"$f":"F35","v":0},{"$f":"G35","v":0}]
[null,"Installed Renewable Energy",null,"Renewable Primary Energy","Adjustment to Eptot","Adjustment to Actual Primary Energy Use","Adjustment to Actual CO2 Emissions"]
["Photovoltaic",{"$f":"B37","v":"Yes"}," ",{"$f":"IF(B103=\"Yes\",B49,0)","v":0},"Accounted for in figures from SBEM",{"$f":"IF(B103=\"Yes\",-B49,0)","v":0},{"$f":"IF(B103=\"Yes\",-B50,0)","v":0}]
["Wind Energy",{"$f":"B38","v":"Yes"}," ",{"$f":"IF(B104=\"Yes\",B57,0)","v":0},"Accounted for in figures from SBEM",{"$f":"IF(B104=\"Yes\",-B57,0)","v":0},{"$f":"IF(B104=\"Yes\",-B58,0)","v":0}]
["Solar Panel","Yes"," ",{"$f":"IF(B105=\"Yes\",B64,0)","v":0},{"$f":"IF(B105=\"Yes\",B64,0)","v":0},"Accounted for in figures from SBEM"]
["Biomass/ Biogas","Yes"," ",{"$f":"IF(B106=\"Yes\",B74,0)","v":0},{"$f":"IF(B106=\"Yes\",(-F29-F33+F74),0)","v":0},{"$f":"IF(B106=\"Yes\",(-F29-F33+F74),0)","v":0},{"$f":"IF(B106=\"Yes\",(-G29-G33+F75),0)","v":0}]
["Combined Heat and Power","Yes"," ",{"$f":"IF(B107=\"Yes\",B85,0)","v":31.020314418604645},{"$f":"IF(B107=\"Yes\",(B81*F86-F82*F85),0)","v":64.907360000000025},{"$f":"IF(B107=\"Yes\",(B81*F86-F82*F85),0)","v":64.907360000000025},{"$f":"IF(B107=\"Yes\",(B81*G86-F82*G85),0)","v":10.949708000000005}]
["Heat Pump Technology","Yes"," ",{"$f":"IF(B108=\"Yes\",B98,0)","v":0},"Accounted for in figures from SBEM"]
[null,null,null,"Guidance Note:"]
["Renewable Primary Energy Epren",{"$f":"SUM(D103:D108)","v":31.020314418604645},"kWh/m2/yr","Complete appropriate sections"]
["Total Primary Energy Eptot",{"$f":"F101+SUM(E103:E108)","v":64.907360000000025},"kWh/m2/yr"]
["Actual Building Primary Energy Use",{"$f":"SUM(F103:F108)+F101","v":64.907360000000025},"kWh/m2/yr"]
["Actual Building Carbon Emissions",{"$f":"SUM(G103:G108)+G101","v":10.949708000000005},"kgCO2/m2/yr"]
[]
[]
["5. Results"]
[null," ",null," "," "," "," "]
[]
["EPC",{"$f":"B112/B24","v":{"$error":"#DIV/0!"}},{"$f":"IF(B119>1,\"Non Compliant\",\"Compliant\")","v":{"$error":"#DIV/0!"}}]
["CPC",{"$f":"B113/B25","v":{"$error":"#DIV/0!"}},{"$f":"IF(B120>1.15,\"Non Compliant\",\"Compliant\")","v":{"$error":"#DIV/0!"}}]
["RER",{"$f":"B110/B111","v":0.4779167480945864},{"$f":"IF(B121<0.2,IF(AND(B121>=0.1,B120<=1.04,B119<=0.9),\"Compliant\",\"Non Compliant\"),\"Compliant\")","v":"Compliant"}]

{"sheet":"Lighting","index":1,"n_rows":98,"n_cols":8,"rows_kept":98,"cut":false,"hidden":false,"merged":[]}
["Zone Name","Wall Area of Zone","Floor Area of Zone, m2","R","Power Density","Design Illuminance","Total Wattage"]
[null,"m2","m2",null,"w/m2/100 lux","lux","Watts"]
["Z1/10 Office",351,179.4,{"$f":"IFERROR(B3/C3,0)","v":1.9565217391304348},{"$f":"((1.93+0.007*D3+0.063*D3^2)/0.8)*60/65","v":2.5209902573796712},500,{"$f":"E3*F3*C3/100","v":2261.3282608695649}]
[null,null,null,{"$f":"IFERROR(B4/C4,0)","v":0},{"$f":"((1.93+0.007*D4+0.063*D4^2)/0.8)*60/65","v":2.2269230769230766},300,{"$f":"E4*F4*C4/100","v":0}]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0," "]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[" "," ",0,{"$f":"IFERROR(B51/C51,0)","v":0},{"$f":"((1.93+0.007*D51+0.063*D51^2)/0.8)*60/65","v":2.2269230769230766},500,{"$f":"E51*F51*C51/100","v":0}]
[null,null,null,{"$f":"IFERROR(B52/C52,0)","v":0},{"$f":"((1.93+0.007*D52+0.063*D52^2)/0.8)*60/65","v":2.2269230769230766},300,{"$f":"E52*F52*C52/100","v":0}]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]
[null,null,null,0,2.2269230769230766,300,0]